# S3 sequence: Pulse red on low battery.
	set.rgb {0,1,2,3}.end 0xff 0x00 0x00
	cycle.1
	delay.w 5000000
L0001:	off
	wait
	jcharge L0001
	jbat L0002 L0001
	jump L0001
L0002:	on
	delay.r 1250
	ramp.1
	swap
	delay.r 10000
	ramp.1
	swap
	jump L0001
