##
## This file is part of the coreboot project.
##
## Copyright (C) 2007 Uwe Hermann <uwe@hermann-uwe.de>
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##
## This program is distributed in the hope that it will be useful,
## but WITHOUT ANY WARRANTY; without even the implied warranty of
## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
## GNU General Public License for more details.
##
## You should have received a copy of the GNU General Public License
## along with this program; if not, write to the Free Software
## Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301 USA
##

chip northbridge/intel/i82810			# Northbridge
  device apic_cluster 0 on			# APIC cluster
    chip cpu/intel/socket_PGA370		# CPU
      device apic 0 on end			# APIC
    end
  end
  device pci_domain 0 on
    device pci 0.0 on end			# Host bridge
    device pci 1.0 on end			# Onboard VGA
    chip southbridge/intel/i82801xx		# Southbridge
      register "ide0_enable" = "1"
      register "ide1_enable" = "1"

      device pci 1e.0 on end			# PCI bridge
      device pci 1f.0 on			# ISA/LPC bridge
        chip superio/winbond/w83627hf		# Super I/O
          device pnp 2e.0 on			# Floppy
            io 0x60 = 0x3f0
            irq 0x70 = 6
            drq 0x74 = 2
          end
          device pnp 2e.1 on			# Parallel port
            io 0x60 = 0x378
            irq 0x70 = 7
            drq 0x74 = 3
          end
          device pnp 2e.2 on			# Com1
            io 0x60 = 0x3f8
            irq 0x70 = 4
          end
          device pnp 2e.3 on			# Com2 (only header on board)
            io 0x60 = 0x2f8
            irq 0x70 = 3
          end
          device pnp 2e.5 on			# PS/2 keyboard/mouse
            io 0x60 = 0x60
            io 0x62 = 0x64
            irq 0x70 = 1			# Keyboard interrupt
            irq 0x72 = 12			# Mouse interrupt
          end
          device pnp 2e.6 off end		# Consumer IR (TODO)
          device pnp 2e.7 on			# Game port / MIDI / GPIO 1
            io 0x60 = 0x201
            io 0x62 = 0x330
            irq 0x70 = 9
          end
          device pnp 2e.8 on end		# GPIO 2
          device pnp 2e.9 on end		# GPIO 3
          device pnp 2e.a on end		# ACPI
          device pnp 2e.b on			# Hardware monitor
            io 0x60 = 0x290
            irq 0x70 = 5
          end
        end
      end
      device pci 1f.1 on end			# IDE
      device pci 1f.2 on end			# USB
      device pci 1f.3 on end			# SMBus
      device pci 1f.5 on end			# AC'97 audio
      device pci 1f.6 on end			# AC'97 modem
    end
  end
end

