chip northbridge/amd/amdk8/root_complex
	device apic_cluster 0 on
		chip cpu/amd/socket_AM2
			device apic 0 on end
		end
end
device pci_domain 0 on
	chip northbridge/amd/amdk8 #mc0
		device pci 18.0 on #  devices on link 0, link 0 == LDT 0
			chip southbridge/nvidia/mcp55
				device pci 0.0 on end # HT
				device pci 1.0 on # LPC
					chip superio/ite/it8716f
						# Floppy and any LDN
						device pnp 2e.0 on
							# Watchdog from CLKIN, CLKIN = 24 MHz
							irq 0x23 = 0x11
							# Serial Flash (SPI only)
							#0x24 = 0x1a
							io 0x60 = 0x3f0
							irq 0x70 = 6
							drq 0x74 = 2
						end
						device pnp 2e.1 on # Com1
							io 0x60 = 0x3f8
							irq 0x70 = 4
						end
						device pnp 2e.2 off # Com2
							io 0x60 = 0x2f8
							irq 0x70 = 3
						end
						device pnp 2e.3 on #  Parallel Port
							io 0x60 = 0x378
							irq 0x70 = 7
						end
						device pnp 2e.4 on #  EC
							io 0x60 = 0x290
							io 0x62 = 0x230
							irq 0x70 = 9
						end
						device pnp 2e.5 on #  Keyboard
							io 0x60 = 0x60
							io 0x62 = 0x64
							irq 0x70 = 1
						end
						device pnp 2e.6 on #  Mouse
							irq 0x70 = 12
						end
						device pnp 2e.7 on #  GPIO, SPI flash
						# pin 84 is not GP10
							irq 0x25 = 0x0
						# pin 21 is GP26, pin 26 is GP21, pin 27 is GP20
							irq 0x26 = 0x43
						# pin 13 is GP35
							irq 0x27 = 0x20
						# pin 70 is not GP46
							#irq 0x28 = 0x0
						# pin 6,3,128,127,126 is GP63,64,65,66,67
							irq 0x29 = 0x81
						# Enable FAN_CTL/FAN_TAC set to 5 (pin 21,23), enable FAN_CTL/FAN_TAC set to 4 (pin 20,22), pin 48 is PCIRST5#, pin91 is PCIRSTIN#, VIN7 is internal voltage divider for VCCH5V, pin 95 is ATXPG, VIN3 is internal voltage divider for VCC5V
							#irq 0x2c = 0x1f
						# Simple I/O base
							io 0x62 = 0x800
						# Serial Flash I/O (SPI only)
							io 0x64 = 0x820
						# watch dog force timeout (parallel flash only)
							#irq 0x71 = 0x1
						# No WDT interrupt
							irq 0x72 = 0x0
						# GPIO pin set 1 disable internal pullup
							irq 0xb8 = 0x0
						# GPIO pin set 5 enable internal pullup
							irq 0xbc = 0x01
						# SIO pin set 1 alternate function
							#irq 0xc0 = 0x0
						# SIO pin set 2 mixed function
							irq 0xc1 = 0x43
						# SIO pin set 3 mixed function
							irq 0xc2 = 0x20
						# SIO pin set 4 alternate function
							#irq 0xc3 = 0x0
						# SIO pin set 1 input mode
							#irq 0xc8 = 0x0
						# SIO pin set 2 input mode
							irq 0xc9 = 0x0
						# SIO pin set 4 input mode
							#irq 0xcb = 0x0
						# Generate SMI# on EC IRQ
							#irq 0xf0 = 0x10
						# SMI# level trigger
							#irq 0xf1 = 0x40
						# HWMON alert beep pin location
							irq 0xf6 = 0x28
						end
						device pnp 2e.8 off #  MIDI
							io 0x60 = 0x300
							irq 0x70 = 10
						end
						device pnp 2e.9 off #  GAME
							io 0x60 = 0x220
						end
						device pnp 2e.a off end #  CIR
					end
				end
				device pci 1.1 on # SM 0
					chip drivers/generic/generic #dimm 0-0-0
						device i2c 50 on end
					end
					chip drivers/generic/generic #dimm 0-0-1
						device i2c 51 on end
					end
					chip drivers/generic/generic #dimm 0-1-0
						device i2c 52 on end
					end
					chip drivers/generic/generic #dimm 0-1-1
						device i2c 53 on end
					end
					chip drivers/generic/generic #dimm 1-0-0
						device i2c 54 on end
					end
					chip drivers/generic/generic #dimm 1-0-1
						device i2c 55 on end
					end
					chip drivers/generic/generic #dimm 1-1-0
						device i2c 56 on end
					end
					chip drivers/generic/generic #dimm 1-1-1
						device i2c 57 on end
					end
				end # SM
				device pci 2.0 on end # USB 1.1
				device pci 2.1 on end # USB 2
				device pci 4.0 on end # IDE
				device pci 5.0 on end # SATA 0
				device pci 5.1 on end # SATA 1
				device pci 5.2 on end # SATA 2
				device pci 6.0 on end # PCI
				device pci 6.1 on end # AUDIO
				device pci 8.0 on end # NIC
				device pci 9.0 off end # N/A
				device pci a.0 on end # PCI E 5
				device pci b.0 on end # PCI E 4
				device pci c.0 on end # PCI E 3
				device pci d.0 on end # PCI E 2
				device pci e.0 on end # PCI E 1
				device pci f.0 on end # PCI E 0
					register "ide0_enable" = "1"
					register "sata0_enable" = "1"
					register "sata1_enable" = "1"
					register "mac_eeprom_smbus" = "3" # 1: smbus under 2e.8, 2: SM0 3: SM1
					register "mac_eeprom_addr" = "0x51"
				end
			end #device pci 18.0
			device pci 18.0 on end # Link 1
			device pci 18.0 on end
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end # mc0
	end # PCI domain

#	chip drivers/generic/debug
#		device pnp 0.0 off end # chip name
#		device pnp 0.1 on end # pci_regs_all
#		device pnp 0.2 on end # mem
#		device pnp 0.3 off end # cpuid
#		device pnp 0.4 on end # smbus_regs_all
#		device pnp 0.5 off end # dual core msr
#		device pnp 0.6 off end # cache size
#		device pnp 0.7 off end # tsc
#		device pnp 0.8 off  end # io
#		device pnp 0.9 off end # io
#	end
end #root_complex
