chip northbridge/amd/amdk8/root_complex
        device apic_cluster 0 on
                chip cpu/amd/socket_940
                        device apic 0 on end
                end
        end

	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on #  northbridge 
				#  devices on link 0, link 0 == LDT 0
				chip southbridge/amd/amd8131
					# the on/off keyword is mandatory
					device pci 0.0 on
                                                device pci 6.0 on end # adaptec
                                                device pci 6.1 on end
                                                device pci 9.0 on end # broadcom 5704
                                                device pci 9.1 on end
					end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 off end
						device pci 1.0 off end
                                                device pci 5.0 on end
                                        #       chip drivers/ati/ragexl
                                                device pci 6.0 on end
                                        #       end
                                                device pci 8.0 on end #intel 10/100
					end
					device pci 1.0 on
						chip superio/winbond/w83627hf
							device pnp 2e.0 on #  Floppy
                	                 			io 0x60 = 0x3f0
                	                			irq 0x70 = 6
                	                			drq 0x74 = 2
							end
                	        			device pnp 2e.1 off #  Parallel Port
                	                 			io 0x60 = 0x378
                	                			irq 0x70 = 7
							end
                	        			device pnp 2e.2 on #  Com1
                	                 			io 0x60 = 0x3f8
                	                			irq 0x70 = 4
							end
                	        			device pnp 2e.3 off #  Com2
                	                 			io 0x60 = 0x2f8
                	                			irq 0x70 = 3
							end
                	        			device pnp 2e.5 on #  Keyboard
                	                 			io 0x60 = 0x60
                	                 			io 0x62 = 0x64
                	                			irq 0x70 = 1
								irq 0x72 = 12
							end
                	                                device pnp 2e.6 off #  CIR
                	                                        io 0x60 = 0x100
                	                                end
                	                                device pnp 2e.7 off #  GAME_MIDI_GIPO1
                	                                        io 0x60 = 0x220
                	                                        io 0x62 = 0x300
                	                                        irq 0x70 = 9
                	                                end  
                	                                device pnp 2e.8 off end #  GPIO2
                	                                device pnp 2e.9 off end #  GPIO3
                	                                device pnp 2e.a off end #  ACPI
                	                                device pnp 2e.b on #  HW Monitor
                	                                        io 0x60 = 0x290
                	                                        irq 0x70 = 5
                	                                end
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.3 on 
#						 chip drivers/generic/generic #dimm 0-0-0
#							 device i2c 50 on end
#						 end
#						 chip drivers/generic/generic #dimm 0-0-1
#							 device i2c 51 on end
#						 end	 
#						 chip drivers/generic/generic #dimm 0-1-0
#							 device i2c 52 on end
#						 end
#						 chip drivers/generic/generic #dimm 0-1-1
#							 device i2c 53 on end
#						 end
#						 chip drivers/generic/generic #dimm 1-0-0
#							 device i2c 54 on end
#						 end
#						 chip drivers/generic/generic #dimm 1-0-1
#							 device i2c 55 on end
#						 end
#						 chip drivers/generic/generic #dimm 1-1-0
#							 device i2c 56 on end
#						 end
#						 chip drivers/generic/generic #dimm 1-1-1
#							 device i2c 57 on end
#						 end
                                        end # acpi
					device pci 1.5 off end
					device pci 1.6 off end
					register "ide0_enable" = "1"
					register "ide1_enable" = "1"
				end
			end #  device pci 18.0 
			
                	device pci 18.0 on end
                	device pci 18.0 on end
			
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end # NB
	end #pci_domain
end

