chip northbridge/amd/amdk8/root_complex
	device apic_cluster 0 on
		chip cpu/amd/socket_940
			device apic 0 on end
		end
	end
	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on #  northbridge 
				#  devices on link 0, link 0 == LDT 0 
				chip southbridge/amd/amd8131
					# the on/off keyword is mandatory
					device pci 0.0 on	# PCIX bridge
						## On board NIC A
						#chip drivers/generic/generic
						#	device pci 3.0 on	
						#		irq 0 = 0x13
						#	end
						#end
						## On board NIC B
						#chip drivers/generic/generic
						#	device pci 4.0 on
						#		irq 0 = 0x13
						#	end
						#end
						## PCI Slot 3
						#chip drivers/generic/generic
						#	device pci 1.0 on
						#		irq 0 = 0x11
						#		irq 1 = 0x12
						#		irq 2 = 0x13
						#		irq 3 = 0x10
						#	end
						#end 
						## PCI Slot 4
						#chip drivers/generic/generic
						#	device pci 2.0 on
						#		irq 0 = 0x12
						#		irq 1 = 0x13
						#		irq 2 = 0x10
						#		irq 3 = 0x11
						#	end
						#end 
					end
					device pci 0.1 on end	# IOAPIC
					device pci 1.0 on 	# PCIX bridge
						## PCI Slot 1
						#chip drivers/generic/generic
						#	device pci 1.0 on
						#		irq 0 = 0x11
						#		irq 1 = 0x12
						#		irq 2 = 0x13
						#		irq 3 = 0x10
						#	end
						#end
						## PCI Slot 2
						#chip drivers/generic/generic
						#	device pci 2.0 on
						#		irq 0 = 0x12
						#		irq 1 = 0x13
						#		irq 2 = 0x10
						#		irq 3 = 0x11
						#	end
						#end 
					end
					device pci 1.1 on end	# IOAPIC
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent of the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on  end	# USB0
						device pci 0.1 on  end	# USB1
						device pci 0.2 off end	# USB 2.0
						device pci 1.0 off end	# LAN
						device pci 6.0 on end # ATI Rage XL
						## PCI Slot 5 (correct?)
						#chip drivers/generic/generic
						#	device pci 5.0 on
						#		irq 0 = 0x11
						#		irq 1 = 0x12
						#		irq 2 = 0x13
						#		irq 3 = 0x10
						#	end
						#end 
						## PCI Slot 6 (correct?)
						#chip drivers/generic/generic
						#	device pci 4.0 on
						#		irq 0 = 0x10
						#		irq 1 = 0x11
						#		irq 2 = 0x12
						#		irq 3 = 0x13
						#	end
						#end 

					end
					# LPC bridge
					device pci 1.0 on
						chip superio/nsc/pc87360
							device	pnp 2e.0 off  # Floppy 
								 io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off  # Parallel Port
								 io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 off # Com 2
								 io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.3 on  # Com 1
								 io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.4 off end # SWC
							device pnp 2e.5 off end # Mouse
							device pnp 2e.6 on  # Keyboard
								 io 0x60 = 0x60
								 io 0x62 = 0x64
								irq 0x70 = 1
							end
							device pnp 2e.7 off end # GPIO
							device pnp 2e.8 off end # ACB
							device pnp 2e.9 off end # FSCM
							device pnp 2e.a off end # WDT  
						end
					end
					device pci 1.1 on end	# IDE
					device pci 1.2 on end	# SMBus 2.0
					device pci 1.3 on 	# System Management
						chip drivers/generic/generic
							#phillips pca9545 smbus mux
							device i2c 70 on 
								# analog_devices adm1026	
								chip drivers/generic/generic
									device i2c 2c on end
								end
							end
							device i2c 70 on end
							device i2c 70 on end
							device i2c 70 on end
						end
						chip drivers/generic/generic #dimm 0-0-0
							device i2c 50 on end
						end
						chip drivers/generic/generic #dimm 0-0-1
							device i2c 51 on end
						end 
						chip drivers/generic/generic #dimm 0-1-0
							device i2c 52 on end
						end 
						chip drivers/generic/generic #dimm 0-1-1
							device i2c 53 on end
						end 
						chip drivers/generic/generic #dimm 1-0-0
							device i2c 54 on end 
						end
						chip drivers/generic/generic #dimm 1-0-1
							device i2c 55 on end
						end 
						chip drivers/generic/generic #dimm 1-1-0
							device i2c 56 on end
						end 
						chip drivers/generic/generic #dimm 1-1-1
							device i2c 57 on end
						end 
					end
					device pci 1.5 off end	# AC97 Audio
					device pci 1.6 on  end	# AC97 Modem
					register "ide0_enable" = "1"
					register "ide1_enable" = "1"
				end
			end #  device pci 18.0 
			
			device pci 18.0 on end # LDT1
			device pci 18.0 on end # LDT2
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end  # chip northbridge/amd/amdk8
		chip northbridge/amd/amdk8
			device pci 19.0 on end
			device pci 19.0 on end
			device pci 19.0 on end
			device pci 19.1 on end
			device pci 19.2 on end
			device pci 19.3 on end
		end
	end 
end

