chip northbridge/via/vt8601
	device pci_domain 0 on
    		device pci 0.0 on end			# Northbridge
#		device pci 0.1 on			# AGP bridge
		#	device pci 0.0 on end		# Integrated VGA
#		end
		chip southbridge/via/vt8231
			register "enable_native_ide" = "0"
			register "enable_com_ports" = "1"
			register "enable_keyboard" = "0"
			device pci 11.0 on              # Southbrdge
				chip superio/winbond/w83627hf
					device pnp 2e.0 on      #  Floppy
					   io 0x60 = 0x3f0
					  irq 0x70 = 6
					  drq 0x74 = 2
					end
					device pnp 2e.1 off     #  Parallel Port
					   io 0x60 = 0x378
					  irq 0x70 = 7
					end
					device pnp 2e.2 on      #  Com1
					   io 0x60 = 0x3f8
					  irq 0x70 = 4
					end
					device pnp 2e.3 off     #  Com2
					   io 0x60 = 0x2f8
					  irq 0x70 = 3
					end
					device pnp 2e.5 on      #  Keyboard
					   io 0x60 = 0x60
					   io 0x62 = 0x64
					  irq 0x70 = 1
					  irq 0x72 = 12
	      				end
				register "com1" = "{CONFIG_TTYS0_BAUD}"
				end
				device pnp 2e.6 off end 	#  CIR
				device pnp 2e.7 off end 	#  GAME_MIDI_GIPO1
				device pnp 2e.8 off end		#  GPIO2
				device pnp 2e.9 off end 	#  GPIO3
				device pnp 2e.a off end		#  ACPI
				device pnp 2e.b on		#  HW Monitor
					io 0x60 = 0x290
				end
			end
			device pci 11.1 on  end		# Ide
			device pci 11.2 off end		# Usb port 0-1
			device pci 11.3 off end		# Usb port 2-3
			device pci 11.4 off end		# ACPI
			device pci 11.5 off end		# AC97 Audio
			device pci 11.6 on  end		# AC97 Modem
          		device pci 12.0 on  end		# Ethernet
        	end
	end

        device apic_cluster 0 on
                chip cpu/via/model_c3
                        device apic 0 on end
                end
        end
end
