chip northbridge/amd/amdk8/root_complex
        device apic_cluster 0 on
                chip cpu/amd/socket_940
                        device apic 0 on end
                end
        end
	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on end # LDT0
			device pci 18.0 on #  northbridge 
				#  devices on link 1, link 1 == LDT 1
				chip southbridge/amd/amd8131
					# the on/off keyword is mandatory
					device pci 0.0 on 
#						chip drivers/lsi/53c1030
#							device pci 4.0 on end
#							device pci 4.1 on end
#							register "fw_address" = "0xfff8c000"
#						end
                                                device pci 9.0 on end #Broadcom
                                                device pci 9.1 on end
					end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 off end
						device pci 1.0 off end
                                                #chip drivers/ati/ragexl
                                                device pci 6.0 on end
                                                #end
                                                device pci 5.0 on end #SiI
					end
					device pci 1.0 on
						chip superio/winbond/w83627hf
							device pnp 2e.0 on #  Floppy
                	                 			io 0x60 = 0x3f0
                	                			irq 0x70 = 6
                	                			drq 0x74 = 2
							end
                	        			device pnp 2e.1 off #  Parallel Port
                	                 			io 0x60 = 0x378
                	                			irq 0x70 = 7
							end
                	        			device pnp 2e.2 on #  Com1
                	                 			io 0x60 = 0x3f8
                	                			irq 0x70 = 4
							end
                	        			device pnp 2e.3 on #  Com2
                	                 			io 0x60 = 0x2f8
                	                			irq 0x70 = 3
							end
                	        			device pnp 2e.5 on #  Keyboard
                	                 			io 0x60 = 0x60
                	                 			io 0x62 = 0x64
                	                			irq 0x70 = 1
								irq 0x72 = 12
							end
                	                                device pnp 2e.6 off #  CIR
                	                                        io 0x60 = 0x100
                	                                end
                	                                device pnp 2e.7 off #  GAME_MIDI_GIPO1
                	                                        io 0x60 = 0x220
                	                                        io 0x62 = 0x300
                	                                        irq 0x70 = 9
                	                                end  
                	                                device pnp 2e.8 off end #  GPIO2
                	                                device pnp 2e.9 off end #  GPIO3
                	                                device pnp 2e.a off end #  ACPI
                	                                device pnp 2e.b on #  HW Monitor
                	                                        io 0x60 = 0x290
                	                                        irq 0x70 = 5
                	                                end
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
                                        device pci 1.3 on 
#                                                chip drivers/i2c/i2cmux # pca9556 smbus mux
#                                                        device i2c 18 on #0 pca9516 2, 1
#	  					                chip drivers/i2c/lm63 #cpu0 temp
#                                                                        device i2c 4c on end
#                                                                end 
#							end
#                                                        device i2c 18 on #1 pca9516 1, 1
#                                                                chip drivers/generic/generic #dimm 1-0-0
#                                                                        device i2c 50 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 1-0-1
#                                                                        device i2c 51 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 1-1-0
#                                                                        device i2c 52 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 1-1-1
#	                                                                device i2c 53 on end
#								end
#                                                        end
#                                                        device i2c 18 on #2 pca9516 1, 2
#                                                                chip drivers/generic/generic #dimm 0-0-0
#                                                                        device i2c 50 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 0-0-1
#                                                                        device i2c 51 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 0-1-0
#                                                                        device i2c 52 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 0-1-1
#                                                                	device i2c 53 on end
#								end
#                                                        end
#                                                        device i2c 18 on #3 pca9516 1, 3
#                                                                chip drivers/generic/generic #dimm 3-0-0
#                                                                        device i2c 50 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 3-0-1
#                                                                        device i2c 51 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 3-1-0
#                                                                        device i2c 52 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 3-1-1
#                                                                	device i2c 53 on end
#								end
#                                                        end
#                                                        device i2c 18 on #4 pca9516 1, 4
#                                                                chip drivers/generic/generic #dimm 2-0-0
#                                                                        device i2c 50 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 2-0-1
#                                                                        device i2c 51 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 2-1-0
#                                                                        device i2c 52 on end
#                                                                end
#                                                                chip drivers/generic/generic #dimm 2-1-1
#                                                                	device i2c 53 on end
#								end
#                                                        end
#                                                        device i2c 18 on #5 pca9516 2, 2
#                                                                chip drivers/i2c/lm63 #cpu1 temp
#                                                                       device i2c 4c on end
#                                                                end
#                                                        end
#                                                        device i2c 18 on #6 pca9516 2, 3
#                                                                chip drivers/i2c/lm63 #cpu2 temp
#                                                                        device i2c 4c on end
#                                                                end
#                                                        end
#                                                        device i2c 18 on #7 pca9516 2, 4
#                                                                chip drivers/i2c/lm63 #cpu3 temp
#                                                                        device i2c 4c on end
#                                                                end
#                                                        end
#                                                end # i2cmux
#                                                chip drivers/i2c/adm1027 # ADM1027 CPU1 vid and System FAN...
#                                                        device i2c 2e on end
#                                                end
#                                                chip drivers/generic/generic # Winbond HWM 0x54 CPU0 vid 
#                                                        device i2c 2a on end
#                                                end
#                                                chip drivers/generic/generic # Winbond HWM 0x92
#                                                        device i2c 49 on end
#                                                end
#                                                chip drivers/generic/generic # Winbond HWM 0x94
#                                                        device i2c 4a on end
#                                                end
#                                                chip drivers/generic/generic # ??
#                                                        device i2c 69 on end
#                                                end
                                        end # acpi
					device pci 1.5 off end
					device pci 1.6 off end
					register "ide0_enable" = "1"
                                        register "ide1_enable" = "1"
				end
			end #  device pci 18.0 
			
                	device pci 18.0 on end
			
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end

	end 
#        chip drivers/generic/debug
#                device pnp 0.0 off end # chip name
#                device pnp 0.1 off end # pci_regs_all
#                device pnp 0.2 off end # mem
#                device pnp 0.3 on end # cpuid
#                device pnp 0.4 off end # smbus_regs_all
#		device pnp 0.5 on end # dual core msr
#		device pnp 0.6 on end # cache size
#		device pnp 0.7 on end # tsc
#        end
end

