{
    "parts": [
        {
            "name": "H9HCNNNBKMMLXR-NEE",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 1,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "H9HCNNNFAMMLXR-NEE",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 4,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 8,
                "ranksPerChannel": 2,
                "speedMbps": 4267
            }
        },
        {
            "name": "K4U6E3S4AA-MGCL",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 1,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "K4UBE3D4AA-MGCL",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 2,
                "speedMbps": 4267
            }
        },
        {
            "name": "MT53E1G32D2NP-046 WT:A",
            "attribs": {
                "densityPerChannelGb": 16,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 1,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "H9HKNNNCRMBVAR-NEH",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "MT53E1G64D4SQ-046 WT:A",
            "attribs": {
                "densityPerChannelGb": 16,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "MT53E512M32D2NP-046 WT:F",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 1,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "NT6AP256T32AV-J2",
            "attribs": {
                "densityPerChannelGb": 4,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 1,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 3733,
                "tckMaxPs": 1250,
                "casLatencies": "14 20 24 28 32"
            }
        },
        {
            "name": "K4U6E3S4AA-MGCR",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 1,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "MT53E512M32D2NP-046 WT:E",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 1,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "H9HCNNNCPMMLXR-NEE",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 2,
                "speedMbps": 4267
            }
        },
        {
            "name": "K4UBE3D4AA-MGCR",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 2,
                "speedMbps": 4267
            }
        },
        {
            "name": "MT53E512M64D4NW-046 WT:E",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "MT53E1G64D8NW-046 WT:E",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 4,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 2,
                "speedMbps": 4267
            }
        },
        {
            "name": "H9HCNNNCRMBLPR-NEE",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "H9HCNNNFBMBLPR-NEE",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 4,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 2,
                "speedMbps": 4267
            }
        },
        {
            "name": "MT53D1G64D4NW-046 WT:A",
            "attribs": {
                "densityPerChannelGb": 16,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        },
        {
            "name": "MT53D512M64D4NW-046 WT:F",
            "attribs": {
                "densityPerChannelGb": 8,
                "banks": 8,
                "channelsPerDie": 2,
                "diesPerPackage": 2,
                "bitWidthPerChannel": 16,
                "ranksPerChannel": 1,
                "speedMbps": 4267
            }
        }
    ]
}
